****************************************************************************
********************** NEC uPD720200 Driver Release Note *******************
****************************************************************************
 Release Note                                                November.2.2009
 
 NEC Electronics uPD720200
 USB 3.0 Host Controller Driver Kit (x86 and x64)
 for Windows XP, Windwos VISTA and Windows 7
 
 Kit Version : 1.0.17.0 : November 2nd, 2009
 Copyright (C) NEC Electronics Corporation 2009 All Rights Reserved
***************************************************************************

IMPORTANT NOTE:
This installer package is generated with InstallShield 2010. If the previous driver package is installed, please uninstall the previous driver package BEFORE installing the new package.


---------------------------------------------------------------------------
Table of Contents
---------------------------------------------------------------------------
1. Release Files
2. How to install
3. History

---------------------------------------------------------------------------
1. Release Files
---------------------------------------------------------------------------
Date       Time       Size     File Name          Version
2009/10/30 14:32      7439KB   setup.exe          1.0.17.0


---------------------------------------------------------------------------
2. Command Line Options
---------------------------------------------------------------------------
1) Normal install

       setup [ENTER]

2) Silent install
 
       setup /s [ENTER]

 -To install this driver package silently, "setup.iss" file is needed.
  This package includes the "setup.iss" in which the following folder 
  path is set.
  "C:\Program Files\NEC Electronics\USB 3.0 Host Controller Driver".

  If you want to change install path, you need to generate setup.iss as
  follows: setup /r /f1".\setup.iss"

3) Checking existence of USB3.0 Host Controller

       setup /v"CHECK_HW_EXIST=1" [ENTER]

 -When this command line option is set, the installer checks existence of 
  the USB3.0 Host Controller(uPD720200). If the uPD720200 is not in the PC,
  this installer does not install the device drivers.

  ##Caution##
  To install the device drivers with this command line option after uninstalling
  the device drivers, it is necessary to restart on the PC.


---------------------------------------------------------------------------
3. History
---------------------------------------------------------------------------
---------------------------------------------------------------------------
 Version 1.0.17.0 : Nobember 2nd, 2009
---------------------------------------------------------------------------

- This version includes the CAT files signed by
  Microsoft Windows Hardware Compatibility Publisher.
  This device driver is complianced with WHQL certification as Unclassified 
  Category on Windows XP, Vista & 7. 
  The Submission ID of WHQL certification is 1371310.

- The following bug was fixed.
   1. Function drivers were not unloaded when disconnectiong gold tree from
      the roothub port of USB3 HC. 

   2. After Warm Reset was issued, enumulation process might fail.

- InstallShield project file, License.rtf and versionDLL were updated.

- The following functions were added.
   1. When Link Errors frequently occur in the SuperSpeed-Port, driver changes 
      the connection from the SuperSpeed to HighSpeed.

   2. Transfer throughput was improved.

   3. Dynamic U1/U2 state control function was disabled. When enabling U1/U2 
      function, the device that SuperSpeed link with host is down was found.
      We decided to disable this function to get interoperability.
      To get certain interoperability, please use the FW version 3.0.2.1 
      released at Nov.2nd 2009 or later.

---------------------------------------------------------------------------
 Version 1.0.14.0 : October 6th, 2009
---------------------------------------------------------------------------

- This version includes the CAT files signed by
  Microsoft Windows Hardware Compatibility Publisher.
  This device driver is complianced with WHQL certification as Unclassified 
  Category on Windows XP, Vista & 7. 
  The Submission ID of WHQL certification is 1358042.

- The following bug fixed.
   1. If the USB Device having multiple Endpoints with same EndpointAddress,
      the USB Device is not enumulated.

   2. The USB2.0 Device connected with mulitiple layered USB2.0 HUB is not detected
      after resuming Sleep and Hibernate.

- Updated InstallShield project file, script file, customDLL & versionDLL.

- Added the following functions to this installer.
   1. Command line option for checking existence of USB3.0 Host Controller.

       /v"CHECK_HW_EXIST=1"

     When this command line option is set, the installer checks existence of 
     the USB3.0 Host Controller(uPD720200). If the uPD720200 is not in the PC,
     this installer does not install the device drivers.

     ##Caution##
     To install the device drivers with this command line option after uninstalling
     the device drivers, it is necessary to restart on the PC.

   2. Previously, this installer does not install device drivers to the PC
      in which device drivers with same version is already installed.
      In this version, it reinstalls the device drivers to the PC.

---------------------------------------------------------------------------
 Version 1.0.12.0 : September 11th, 2009
---------------------------------------------------------------------------
- Updated End User Licence Agreement.

- This version includes the CAT files signed by
  Microsoft Windows Hardware Compatibility Publisher.
  This device driver is complianced with WHQL certification as Unclassified 
  Category on Windows XP, Vista & 7. 
  The Submission ID of WHQL certification is 1349589.

- This package includes "Install Shield 2010 Project Files" in the EXE folder
  with which any cusotmers can customize install package.

- Installer Wizard Messages, "nusb3mon.exe" and "nusb3utl.exe" support 
  the following languages.

  LCID : Language
   0401 : Arabic
   0404 : Traditional Chinese
   0405 : Czech
   0406 : Danish
   0407 : German
   0408 : Greek
   0409 : English
   040A : Spanish (Traditional)
   040B : Finnish
   040C : French
   040D : Hebrew
   040E : Hungarian
   0410 : Italian
   0411 : Japanese
   0412 : Korean
   0413 : Dutch
   0414 : Norwegian (Bokmal)
   0415 : Polish
   0416 : Portuguese (Brazilian)
   0419 : Russian
   041B : Slovak
   041D : Swedish
   041E : Thai
   041F : Turkish
   0424 : Slovenian
   0804 : Simplified Chinese
   0816 : Portuguese(Standard)
   0C04 : Chinese (Hong Kong)
   0C0A : Spanish (Modern)
   2C0A : Spanish (Latin America)

- The following bug fixed.
   1. Bluescreen sometimes occurs when starting WebCam application.

   2. The mouse supported SelectiveSuspend function does not work when 
      it wakes up from suspend state.

   3. Can't access CD-ROM Media in a Blu-Ray Drive.

- Optimized SS/HS bulk transfer performance

---------------------------------------------------------------------------
 Version 1.0.10.0 : August 26th, 2009
---------------------------------------------------------------------------
- This version includes the CAT files signed by
  Microsoft Windows Hardware Compatibility Publisher.
  This device driver is complianced with WHQL certification as Unclassified 
  Category on Windows XP, Vista & 7. 
  The Submission ID of WHQL certification is 1346130.

- All of files except for the CAT files are same as Version1.0.10.0 Beta2

---------------------------------------------------------------------------
 Version 1.0.10.0Beta2 : August 24th, 2009
---------------------------------------------------------------------------
- This version includes Microsoft TestSigned CAT Files.
  Note: If this driver package is used on x64 Windows Vista/7,
        need to set the following command. 
        >bcdedit -set TESTSIGNING ON

- This installer package is generated with the InstallShield2010.
  If the previous driver package(v0.X.X.X , v1.0.1.0 or v1.0.7.0) is installed,
  please uninstall the previous driver package and install new package.

- Installer Wizard Messages, "nusb3mon.exe" and "nusb3utl.exe" support 
  the following languages.

  LCID : Language
   404 : Traditional Chinese
   407 : German
   409 : English
   40A : Spanish
   40C : French
   410 : Italian
   411 : Japanese
   412 : Korean
   413 : Dutch
   804 : Simplified Chinese
   816 : Portuguese(Standard)

- The following bug fixed.
   1. Some hub devices does not detected after resuming Sleep and Hibernate.

   2. Bluescreen occurs after resuming Sleep and Hibernate.

- Known issue. This issue will fixed at next version.
   1. Bluescreen sometimes occurs when strting WebCam application.

---------------------------------------------------------------------------
 Version 1.0.7.0Beta : July 17th, 2009
---------------------------------------------------------------------------
- The following bug fixed.

1. USB Devices are not detected after resuming from Sleep and Hibernate.

2. Bluescreen occurs after resuming from Sleep and Hibernate.

3. USB-VGA Devices does not work correctly.

4. The message that bandwidth is getting low might not be indicated.

-The following function Added
1. Add a Vender Defined Command. 

---------------------------------------------------------------------------
 Version 1.0.1.0Beta : June 15th, 2009
---------------------------------------------------------------------------
- This package includes the following applications.
  1. nusb3mon.exe
  This application provides the following function 
  USB3.0 Specificatin Section 11.1 indicates the follwoing function.
  To address the situation where a USB 3.0 device is connected to a
  USB 2.0-only port on a USB 3.0- capable host, after establishing a
  USB 2.0 high-speed connection with the device, it is recommended
  that the host inform the user that the device will support
  SuperSpeed operation if it is moved to a USB 3.0-capable port on the
  same host. If a USB 3.0 device is connected to a USB 3.0- capable
  host via a USB 2.0 hub, it is recommended that the host inform the
  user that the device will support SuperSpeed operation if it is
  moved to an appropriate host port or if the hub is replaced with a
  USB 3.0 hub.

  2. nusb3ver.exe 
  This application provides functions that shows Driver Version 
  and Firmware Version.

- The following bug fixed.

1. Function driver is not unloaded after resuming from Sleep and Hibernate.

2. USB Remote wake up function is not worked correctly.

3. Bluescreen occured when repeating hot-pulg of FS-Speaker Device 
   that is connected with HS-Hub that is connected with USB3.0 HC.

---------------------------------------------------------------------------
 Version 0.9.12.0Beta : May 29th, 2009
---------------------------------------------------------------------------
- Changed installer package configuration.

  1. EXE type
     *All files are included in the EXE file.
     *Combined x86 and x64 in one package.

  2. ZIP type
     *Conposed of 3 contents, setup.exe, x86 folder and x64 folder.
     *All files for x86 are in x86 folder.
     *All files for x64 are in x64 folder.
     *Setup.exe installs drivers automatically.

---------------------------------------------------------------------------
 Version 0.9.12.0Beta : May 27th, 2009
---------------------------------------------------------------------------
- The following bug fixed.

1. Function driver is not unloaded after resuming from Sleep and Hibernate.

2. When repeating hot-pulg of a USB2.0 device, the device is not detected.

3. When connecting two USB Devices and after resuming from Sleep and Hibernate,
   both devices is not detected.

4. Bluescreen occuerd when USB-VGA device is running.

5. Dual Display mode of a USB-VGA device can't be operated.

---------------------------------------------------------------------------
 Version 0.9.4.0Beta : March 27th, 2009
---------------------------------------------------------------------------
- Support for Super Speed Transactions

---------------------------------------------------------------------------
 Version 0.9.3.0Beta : March 9th, 2009
---------------------------------------------------------------------------
- The following bug fixed.

1. If the system is booted up with a USB device already present on the USB 
   port, the USB port is in-operative and cannot be recovered even if the 
   USB device is unplugged and then plugged back in.

---------------------------------------------------------------------------
 Version 0.9.0.0Beta : February 9th, 2009
---------------------------------------------------------------------------
- First Beta Version Release
---------------------------------------------------------------------------
