; PCI60806A.INF
; Driver for PCI60806A (PCI=>DUAL SERIAL,PCI=>SERIAL AND PARALLEL,PCI=>DUAL SERIAL AND PARALLEL,PCI=>QUAD SERIAL)
; For 98/ME/2K/XP/VISTA/SERVER/64bit XP/64bit VISTA
; Copyright (C) PCI 2008-2012
; VER V1.1

[Version]
Signature=$CHICAGO$
Class=MultiFunction
ClassGUID={4d36e971-e325-11ce-bfc1-08002be10318}
Provider=%PCI60806A%
DriverVer=01/01/2010,1.1.2010.1

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%PCI60806A%=PCI60806A
%PCI60806A%=PCI60806A,NTAMD64
%PCI60806A%=PCI60806A,NTIA64

[PCI60806A]
%PCI60806A_PORT_SS%=PCI60806ASS_inst, PCI\VEN_4651&DEV_3273
%PCI60806A_PORT_SS%=PCI60806ASS_inst, PCI\VEN_4651&DEV_3273&SUBSYS_32734651
%PCI60806A_PORT_SP%=PCI60806ASP_inst, PCI\VEN_4651&DEV_7073
%PCI60806A_PORT_SP%=PCI60806ASP_inst, PCI\VEN_4651&DEV_7073&SUBSYS_70734651
%PCI60806A_PORT_SSP%=PCI60806ASSP_inst, PCI\VEN_4651&DEV_5073
%PCI60806A_PORT_SSP%=PCI60806ASSP_inst, PCI\VEN_4651&DEV_5073&SUBSYS_32734651
%PCI60806A_PORT_SSP_RA%=PCI60806ASPR_inst, PCI\VEN_4651&DEV_5046
%PCI60806A_PORT_SSP_RA%=PCI60806ASPR_inst, PCI\VEN_4651&DEV_5046&SUBSYS_50464651
%PCI60806A_PORT_4S3%=PCI60806A4S3_inst, PCI\VEN_4651&DEV_3473
%PCI60806A_PORT_4S3%=PCI60806A4S3_inst, PCI\VEN_4651&DEV_3473&SUBSYS_34734651

[PCI60806A.NTAMD64]
%PCI60806A_PORT_SS%=PCI60806ASS_inst, PCI\VEN_4651&DEV_3273
%PCI60806A_PORT_SS%=PCI60806ASS_inst, PCI\VEN_4651&DEV_3273&SUBSYS_32734651
%PCI60806A_PORT_SP%=PCI60806ASP_inst, PCI\VEN_4651&DEV_7073
%PCI60806A_PORT_SP%=PCI60806ASP_inst, PCI\VEN_4651&DEV_7073&SUBSYS_70734651
%PCI60806A_PORT_SSP%=PCI60806ASSP_inst, PCI\VEN_4651&DEV_5073
%PCI60806A_PORT_SSP%=PCI60806ASSP_inst, PCI\VEN_4651&DEV_5073&SUBSYS_32734651
%PCI60806A_PORT_SSP_RA%=PCI60806ASPR_inst, PCI\VEN_4651&DEV_5046
%PCI60806A_PORT_SSP_RA%=PCI60806ASPR_inst, PCI\VEN_4651&DEV_5046&SUBSYS_50464651
%PCI60806A_PORT_4S3%=PCI60806A4S3_inst, PCI\VEN_4651&DEV_3473
%PCI60806A_PORT_4S3%=PCI60806A4S3_inst, PCI\VEN_4651&DEV_3473&SUBSYS_34734651

[PCI60806A.NTIA64]
%PCI60806A_PORT_SS%=PCI60806ASS_inst, PCI\VEN_4651&DEV_3273
%PCI60806A_PORT_SS%=PCI60806ASS_inst, PCI\VEN_4651&DEV_3273&SUBSYS_32734651
%PCI60806A_PORT_SP%=PCI60806ASP_inst, PCI\VEN_4651&DEV_7073
%PCI60806A_PORT_SP%=PCI60806ASP_inst, PCI\VEN_4651&DEV_7073&SUBSYS_70734651
%PCI60806A_PORT_SSP%=PCI60806ASSP_inst, PCI\VEN_4651&DEV_5073
%PCI60806A_PORT_SSP%=PCI60806ASSP_inst, PCI\VEN_4651&DEV_5073&SUBSYS_32734651
%PCI60806A_PORT_SSP_RA%=PCI60806ASPR_inst, PCI\VEN_4651&DEV_5046
%PCI60806A_PORT_SSP_RA%=PCI60806ASPR_inst, PCI\VEN_4651&DEV_5046&SUBSYS_50464651
%PCI60806A_PORT_4S3%=PCI60806A4S3_inst, PCI\VEN_4651&DEV_3473
%PCI60806A_PORT_4S3%=PCI60806A4S3_inst, PCI\VEN_4651&DEV_3473&SUBSYS_34734651

[StandardMF.Reg]
HKR,,DevLoader,,*CONFIGMG
HKR,,Enumerator,,*CONFIGMG
HKR,,CMDrivFlags,1,03,00,00,00

;;2S
; WIN98/ME
[PCI60806ASS_inst]
AddReg=StandardMF.Reg

[PCI60806ASS_inst.HW]
AddReg=PCI60806ASS_inst.RegHW

[PCI60806ASS_inst.RegHW]
HKR,Child0000,HardwareID,,MF\PCI3273_COM_0
HKR,Child0000,ResourceMap,1,00,01
HKR,Child0001,HardwareID,,MF\PCI3273_COM_1
HKR,Child0001,ResourceMap,1,00,02

; WIN2K
[PCI60806ASS_inst.NT]
Include = mf.inf
Needs = MFINSTALL.mf

[PCI60806ASS_inst.NT.HW]
AddReg=PCI60806ASS_inst.NT.RegHW

[PCI60806ASS_inst.NT.Services]
Include = mf.inf
Needs = MFINSTALL.mf.Services
       
[PCI60806ASS_inst.NT.RegHW]
HKR,Child0000,HardwareID,,MF\PCI3273_COM_0
HKR,Child0000,ResourceMap,1,00,04
HKR,Child0001,HardwareID,,MF\PCI3273_COM_1
HKR,Child0001,ResourceMap,1,02,04

;;1S1P
; WIN98/ME
[PCI60806ASP_inst]
AddReg=StandardMF.Reg

[PCI60806ASP_inst.HW]
AddReg=PCI60806ASP_inst.RegHW

[PCI60806ASP_inst.RegHW]
;HKR,Child0000,HardwareID,,MF\PCI7073_COM_0
HKR,Child0000,ResourceMap,1,00,01
HKR,Child0001,HardwareID,,MF\PCI7073_LPT_0
HKR,Child0001,ResourceMap,1,00,02

; WIN2K
[PCI60806ASP_inst.NT]
Include = mf.inf
Needs = MFINSTALL.mf

[PCI60806ASP_inst.NT.HW]
AddReg=PCI60806ASP_inst.NT.RegHW

[PCI60806ASP_inst.NT.Services]
Include = mf.inf
Needs = MFINSTALL.mf.Services

[PCI60806ASP_inst.NT.RegHW]
;HKR,Child0000,HardwareID,,MF\PCI7073_COM_0
;HKR,Child0000,ResourceMap,1,00,04
HKR,Child0001,HardwareID,,MF\PCI7073_LPT_0
HKR,Child0001,ResourceMap,1,02,04

;;2S1P
; WIN98/ME
[PCI60806ASSP_inst]
AddReg=StandardMF.Reg

[PCI60806ASSP_inst.HW]
AddReg=PCI60806ASSP_inst.RegHW

[PCI60806ASSP_inst.RegHW]
HKR,Child0000,HardwareID,,MF\PCI5073_COM_0
HKR,Child0000,ResourceMap,1,00,01
HKR,Child0001,HardwareID,,MF\PCI5073_COM_1
HKR,Child0001,ResourceMap,1,00,02
HKR,Child0002,HardwareID,,MF\PCI5073_LPT_0
HKR,Child0002,ResourceMap,1,00,03

; WIN2K
[PCI60806ASSP_inst.NT]
Include = mf.inf
Needs = MFINSTALL.mf

[PCI60806ASSP_inst.NT.HW]
AddReg=PCI60806ASSP_inst.NT.RegHW

[PCI60806ASSP_inst.NT.Services]
Include = mf.inf
Needs = MFINSTALL.mf.Services

[PCI60806ASSP_inst.NT.RegHW]
HKR,Child0000,HardwareID,,MF\PCI5073_COM_0
HKR,Child0000,ResourceMap,1,00,08
HKR,Child0001,HardwareID,,MF\PCI5073_COM_1
HKR,Child0001,ResourceMap,1,02,08
HKR,Child0002,HardwareID,,MF\PCI5073_LPT_0
HKR,Child0002,ResourceMap,1,04,08

;;2S1P_ReserveAddress
; WIN98/ME
[PCI60806ASPR_inst]
AddReg=StandardMF.Reg

[PCI60806ASPR_inst.HW]
AddReg=PCI60806ASPR_inst.RegHW

[PCI60806ASPR_inst.RegHW]
HKR,Child0000,HardwareID,,MF\PCI5046_COM_0
HKR,Child0000,ResourceMap,1,00,01
HKR,Child0001,HardwareID,,MF\PCI5046_COM_1
HKR,Child0001,ResourceMap,1,00,02
HKR,Child0002,HardwareID,,MF\PCI5046_LPT_0
HKR,Child0002,ResourceMap,1,00,03

; WIN2K
[PCI60806ASPR_inst.NT]
Include = mf.inf
Needs = MFINSTALL.mf

[PCI60806ASPR_inst.NT.HW]
AddReg=PCI60806ASPR_inst.NT.RegHW

[PCI60806ASPR_inst.NT.Services]
Include = mf.inf
Needs = MFINSTALL.mf.Services

[PCI60806ASPR_inst.NT.RegHW]
HKR,Child0000,HardwareID,,MF\PCI5046_COM_0
HKR,Child0000,ResourceMap,1,00,08
HKR,Child0001,HardwareID,,MF\PCI5046_COM_1
HKR,Child0001,ResourceMap,1,02,08
HKR,Child0002,HardwareID,,MF\PCI5046_LPT_0
HKR,Child0002,ResourceMap,1,04,08

;;4S
; WIN98/ME
[PCI60806A4S3_inst]
AddReg=StandardMF.Reg

[PCI60806A4S3_inst.HW]
AddReg=PCI60806A4S3_inst.RegHW

[PCI60806A4S3_inst.RegHW]
HKR,Child0000,HardwareID,,MF\PCI3473_COM_0
HKR,Child0000,ResourceMap,1,00,01
HKR,Child0001,HardwareID,,MF\PCI3473_COM_1
HKR,Child0001,ResourceMap,1,00,02
HKR,Child0002,HardwareID,,MF\PCI3473_COM_2
HKR,Child0002,ResourceMap,1,00,03
HKR,Child0003,HardwareID,,MF\PCI3473_COM_3
HKR,Child0003,ResourceMap,1,00,04

; WIN2K
[PCI60806A4S3_inst.NT]
Include = mf.inf
Needs = MFINSTALL.mf

[PCI60806A4S3_inst.NT.HW]
AddReg=PCI60806A4S3_inst.NT.RegHW

[PCI60806A4S3_inst.NT.Services]
Include = mf.inf
Needs = MFINSTALL.mf.Services

[PCI60806A4S3_inst.NT.RegHW]
HKR,Child0000,HardwareID,,MF\PCI3473_COM_0
HKR,Child0000,ResourceMap,1,00,08
HKR,Child0001,HardwareID,,MF\PCI3473_COM_1
HKR,Child0001,ResourceMap,1,02,08
HKR,Child0002,HardwareID,,MF\PCI3473_COM_2
HKR,Child0002,ResourceMap,1,04,08
HKR,Child0003,HardwareID,,MF\PCI3473_COM_3
HKR,Child0003,ResourceMap,1,06,08

[Strings]
PCI60806A= "PCI"
PCI60806A_PORT_SS = "PCI PCI=>DUAL SERIAL"
PCI60806A_PORT_SP = "PCI PCI=>PARALLEL"
PCI60806A_PORT_SSP = "PCI PCI=>DUAL SERIAL&&PARALLEL"
PCI60806A_PORT_SSP_RA = "PCI PCI=>DUAL SERIAL&&PARALLEL_RA"
PCI60806A_PORT_4S3 = "PCI PCI=>QUAD SERIAL"
