This installation guide describes the procedures to install and uninstall PCI60806A PCI to two serial ports,one serial and one parport,
two serial ports and one parport,four serial ports in Linux platform.
1-install and uninstall PCI60806A PCI boards

(1)-install
<1>-copy pci60806a.o to /usr/sbin
<2>-Add /usr/sbin/pci60806a at the end of the /etc/rc.d/rc.local.
<3>-reboot
if you inster two serials port board
The ttyS2 and ttyS3 are ready for application.

if you inster one serial port and one parport port board
The ttyS2 and LPT1 or LPT2 ready for application.

if you inster four serials port board
The ttyS2 ttyS3 ttyS4 and ttyS5 are ready for application.

if you inster two serials port and aone parport port board
The ttyS2 ttyS3 and LPT1 or LPT2 are ready for application.


(2)-uninstall
(1)-Remove /usr/sbin/pci60806a at the end of the /etc/rc.d/rc.local.
(2)-Remove /usr/sbin/pci60806a.o





